IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [ContentGUID: 29177240-8994-4c89-954b-ba6f97971b8b, VersionGUID: cf7426b5-a7cc-4948-905a-2626745d61fd, NumberOfSaves: 76]"
Description: "CoordinateReference [CoordinateBase: Coordinate condivise]"
Description: "ExchangeRequirement [Structural]"
File name: "PFTE_10BIM_090_STR_SP_010_00_Modello disciplinare dello stato di progetto.ifc"
Time stamp: "2026-06-22T13:26:49+01:00"
Preprocessor: "ODA SDAI 24.12"
Originating system: "Autodesk Revit 25.4.50.35 (ITA) - IFC 25.4.50.35"
Application: "Autodesk Revit 2025 (ITA)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ITA)"

People and organizations
  Person "lucchesiU2UCH" of Organization (no name given)
  Owner history of Person "lucchesiU2UCH" of Organization (no name given) | application "Autodesk Revit 2025 (ITA)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ITA)" | change NOCHANGE | created 1782125633 (2026-06-22T10:53:53Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  THERMALTRANSMITTANCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nome del progetto" | phase "Stato del progetto"
  IFCSITE "Default" | latitude 43° 50′ 31.182861″ | longitude 10° 30′ 41.119766″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Immettere l'indirizzo", "43", "84199523925781", "10", "511422157287598"
      IFCBUILDINGSTOREY "Livello 0" | long name "Livello 0" | object type "Livello:Estremità 8 mm" | elevation -749.
        contains 46 elements
          6 x IFCFOOTING | type IFCFOOTINGTYPE "Muro di base:Generico - 400 mm" | object type "Muro di base:Generico - 400 mm" | FOOTING_BEAM | names: "Muro di base:Generico - 400 mm:387519", "Muro di base:Generico - 400 mm:387531", "Muro di base:Generico - 400 mm:389477" (+3 more) | material: "Muro di default" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting, Qto_FootingBaseQuantities
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Muro di base:Generico - 350 mm" | object type "Muro di base:Generico - 350 mm" | FOOTING_BEAM | names: "Muro di base:Generico - 350 mm:387525" | material: "Muro di default" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting, Qto_FootingBaseQuantities
          1 x IFCRAMP | type IFCRAMPTYPE "Pavimento:Rampa strutturale_CLS_2" | object type "Pavimento:Rampa strutturale_CLS_2" | STRAIGHT_RUN_RAMP | names: "Pavimento:Rampa strutturale_CLS_2:500399" | material: "Calcestruzzo, gettato in opera" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RampCommon, Pset_RampFlightCommon
          1 x IFCWALL | type IFCWALLTYPE "Mura:Mura" | object type "Mura:Mura" | SOLIDWALL | names: "Mura:Mura:532184" | material: "Muro di default" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon, Qto_WallBaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:508851" | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          1 x IFCBEAM | object type "Rafter" | names: "Rafter" | descriptions: "AGB AB{F3B0E60E-398C-4151-853C-68F2BDB22AF9}" | property sets: ProfileProperties
          2 x IFCCOLUMN | object type "Rafter" | names: "Rafter" | descriptions: "AGB CSP{145059FE-AD64-46BE-9E0D-BE241F7C94FD}" | property sets: ProfileProperties
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:390929", "Pilastro RHS (EN 10210-2):RHS120x80x5:391458", "Pilastro RHS (EN 10210-2):RHS120x80x5:518389" (+1 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          1 x IFCPLATE | object type "-" | names: "-" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          25 x IFCMECHANICALFASTENER | object type "-"
          3 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "Livello 1" | long name "Livello 1" | object type "Livello:Estremità 8 mm" | elevation -715.
        contains 33 elements
          1 x IFCRAMP | type IFCRAMPTYPE "Pavimento:Rampa strutturale_CLS_1" | object type "Pavimento:Rampa strutturale_CLS_1" | STRAIGHT_RUN_RAMP | names: "Pavimento:Rampa strutturale_CLS_1:499601" | material: "Calcestruzzo, gettato in opera" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RampCommon, Pset_RampFlightCommon
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:390638", "Pilastro RHS (EN 10210-2):RHS120x80x5:390625", "Pilastro RHS (EN 10210-2):RHS120x80x5:511369" (+2 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          23 x IFCBEAM | object type "Rafter" | names: "Rafter" | descriptions: "AGB AB{F3B0E60E-398C-4151-853C-68F2BDB22AF9}" | property sets: ProfileProperties
          2 x IFCCOLUMN | object type "Rafter" | names: "Rafter" | descriptions: "AGB CSP{145059FE-AD64-46BE-9E0D-BE241F7C94FD}" | property sets: ProfileProperties
          2 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "-7.00m" | long name "-7.00m" | object type "Livello:Estremità 8 mm" | elevation -700.
        contains 59 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:391297" | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          13 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro SHS (EN 10210-2):SHS120x5" | object type "SHS120x5" | names: "Pilastro SHS (EN 10210-2):SHS120x5:387374", "Pilastro SHS (EN 10210-2):SHS120x5:387287", "Pilastro SHS (EN 10210-2):SHS120x5:387286" (+10 more) | descriptions: "FRQ{C67B81B0-1E59-4DC6-8B30-115CE3698D26}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:423162" | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          11 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:501245", "Pilastro RHS (EN 10210-2):RHS120x80x5:504613", "Pilastro RHS (EN 10210-2):RHS120x80x5:504625" (+8 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          10 x IFCMECHANICALFASTENER | object type "-"
          23 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "Livello 2" | long name "Livello 2" | object type "Livello:Estremità 8 mm" | elevation -690.
        contains 111 elements
          16 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "RHS (EN 10210-2):RHS120x80x5:392313", "RHS (EN 10210-2):RHS120x80x5:392309", "RHS (EN 10210-2):RHS120x80x5:388895" (+13 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          32 x IFCBEAM | object type "Rafter" | names: "Rafter" | descriptions: "AGB AB{1D08A026-D2C0-42D8-B82A-53E07B6829BA}", "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}" | property sets: ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "Barre circolari:RB 12" | object type "RB 12" | names: "Barre circolari:RB 12:501102", "Barre circolari:RB 12:437249" | descriptions: "AGB ASB{326B3597-30B9-466E-ADCF-3E81CE34C0BC}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "Barre circolari:RB 12" | object type "RB 12" | names: "Barre circolari:RB 12:501101", "Barre circolari:RB 12:437248" | descriptions: "AGB ASB{326B3597-30B9-466E-ADCF-3E81CE34C0BC}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          4 x IFCPLATE | object type "Gusset" | names: "Gusset" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          4 x IFCMECHANICALFASTENER | object type "Bolt#2"
          11 x IFCMECHANICALFASTENER | object type "-"
          40 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "-6.33m" | long name "-6.33m" | object type "Livello:Estremità 8 mm" | elevation -633.
        contains 116 elements
          34 x IFCBEAM | object type "Angle_Cleat#2" | names: "Angle_Cleat#2" | descriptions: "AGB AB{1D08A026-D2C0-42D8-B82A-53E07B6829BA}", "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}" | property sets: ProfileProperties
          1 x IFCBEAM | object type "Rafter" | names: "Rafter" | descriptions: "AGB CSP{145059FE-AD64-46BE-9E0D-BE241F7C94FD}" | property sets: ProfileProperties
          4 x IFCPLATE | object type "Gusset" | names: "Gusset" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          4 x IFCMECHANICALFASTENER | object type "Bolt#1"
          23 x IFCMECHANICALFASTENER | object type "-"
          50 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "Livello 3" | long name "Livello 3" | object type "Livello:Estremità 8 mm" | elevation -486.00000000000006
        contains 222 elements
          34 x IFCBEAM | object type "Angle_Cleat#2" | names: "Angle_Cleat#2" | descriptions: "AGB AB{1D08A026-D2C0-42D8-B82A-53E07B6829BA}", "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}" | property sets: ProfileProperties
          5 x IFCBEAM | object type "Rafter" | names: "Rafter" | descriptions: "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}", "AGB CSP{145059FE-AD64-46BE-9E0D-BE241F7C94FD}" | property sets: ProfileProperties
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:510116" | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          17 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "RHS (EN 10210-2):RHS120x80x5:392327", "RHS (EN 10210-2):RHS120x80x5:511428", "RHS (EN 10210-2):RHS120x80x5:389306" (+14 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235"; "Soletta metallica" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "Barre circolari:RB 12" | object type "RB 12" | names: "Barre circolari:RB 12:435298", "Barre circolari:RB 12:501099" | descriptions: "AGB ASB{326B3597-30B9-466E-ADCF-3E81CE34C0BC}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "Barre circolari:RB 12" | object type "RB 12" | names: "Barre circolari:RB 12:435924", "Barre circolari:RB 12:501100" | descriptions: "AGB ASB{326B3597-30B9-466E-ADCF-3E81CE34C0BC}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:396569", "Pilastro RHS (EN 10210-2):RHS120x80x5:396570" | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          8 x IFCPLATE | object type "Gusset" | names: "Gusset" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          11 x IFCPLATE | object type "-" | names: "-" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 100.) | property sets: Pset_PlateCommon
          2 x IFCPLATE | object type "Endplate" | names: "Endplate" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          4 x IFCMECHANICALFASTENER | object type "Bolt#2"
          4 x IFCMECHANICALFASTENER | object type "Bolt#1"
          37 x IFCMECHANICALFASTENER | object type "-"
          93 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "Livello 4" | long name "Livello 4" | object type "Livello:Estremità 8 mm" | elevation -283.
        contains 81 elements
          19 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "RHS (EN 10210-2):RHS120x80x5:389334", "RHS (EN 10210-2):RHS120x80x5:392339", "RHS (EN 10210-2):RHS120x80x5:391697" (+16 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          4 x IFCBEAM | object type "Rafter" | names: "Rafter" | descriptions: "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}" | property sets: ProfileProperties
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "Pilastro RHS (EN 10210-2):RHS120x80x5:396271", "Pilastro RHS (EN 10210-2):RHS120x80x5:396640", "Pilastro RHS (EN 10210-2):RHS120x80x5:396641" (+1 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "Barre circolari:RB 12" | object type "RB 12" | names: "Barre circolari:RB 12:501103", "Barre circolari:RB 12:437355" | descriptions: "AGB ASB{326B3597-30B9-466E-ADCF-3E81CE34C0BC}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "Barre circolari:RB 12" | object type "RB 12" | names: "Barre circolari:RB 12:501104", "Barre circolari:RB 12:437356" | descriptions: "AGB ASB{326B3597-30B9-466E-ADCF-3E81CE34C0BC}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          11 x IFCMEMBER | type IFCMEMBERTYPE "RHS (EN 10210-2):RHS60x40x4" | object type "RHS60x40x4" | names: "RHS (EN 10210-2):RHS60x40x4:532963", "RHS (EN 10210-2):RHS60x40x4:536586", "RHS (EN 10210-2):RHS60x40x4:536594" (+8 more) | descriptions: "FRQ{50E91A94-FE19-49F6-AD49-8D63460E1796}" | material: "Acciaio strutturale - S235" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          4 x IFCPLATE | object type "Gusset" | names: "Gusset" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          4 x IFCMECHANICALFASTENER | object type "Bolt#2"
          3 x IFCMECHANICALFASTENER | object type "-"
          28 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "-2.72m" | long name "-2.72m" | object type "Livello:Estremità 8 mm" | elevation -272.
        contains 332 elements
          44 x IFCBEAM | object type "Purlin_Cleat" | names: "Purlin_Cleat" | descriptions: "AGB AB{1D08A026-D2C0-42D8-B82A-53E07B6829BA}" | property sets: ProfileProperties
          24 x IFCBEAM | object type "Angle_Cleat#2" | names: "Angle_Cleat#2" | descriptions: "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}" | property sets: ProfileProperties
          4 x IFCPLATE | object type "Gusset" | names: "Gusset" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          13 x IFCPLATE | object type "Endplate" | names: "Endplate" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.); layers "Soletta metallica" ("Soletta metallica" 8.5) | property sets: Pset_PlateCommon
          2 x IFCPLATE | object type "Stiffener#1" | names: "Stiffener#1" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          2 x IFCPLATE | object type "Stiffener#0" | names: "Stiffener#0" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 10.) | property sets: Pset_PlateCommon
          11 x IFCPLATE | object type "-" | names: "-" | descriptions: "-" | material: layers "Soletta metallica" ("Soletta metallica" 100.) | property sets: Pset_PlateCommon
          4 x IFCMECHANICALFASTENER | object type "Bolt#1"
          68 x IFCMECHANICALFASTENER | object type "-"
          160 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "Livello 5" | long name "Livello 5" | object type "Livello:Estremità 8 mm" | elevation -123.99999999999999
        contains 208 elements
          1 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS (EN 10210-2):RHS180x100x5" | JOIST | names: "RHS (EN 10210-2):RHS180x100x5:515616" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          5 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS (EN 10210-2):RHS180x100x5" | JOIST | names: "RHS (EN 10210-2):RHS180x100x5:515863", "RHS (EN 10210-2):RHS180x100x5:515993", "RHS (EN 10210-2):RHS180x100x5:516271" (+2 more) | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS (EN 10210-2):RHS180x100x5" | JOIST | names: "RHS (EN 10210-2):RHS180x100x5:516161" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS (EN 10210-2):RHS180x100x5" | JOIST | names: "RHS (EN 10210-2):RHS180x100x5:516808" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS (EN 10210-2):RHS180x100x5" | JOIST | names: "RHS (EN 10210-2):RHS180x100x5:516895" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS (EN 10210-2):RHS180x100x5" | JOIST | names: "RHS (EN 10210-2):RHS180x100x5:517122" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          60 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS100x50x5" | object type "RHS100x50x5" | names: "RHS (EN 10210-2):RHS100x50x5:441152", "RHS (EN 10210-2):RHS100x50x5:441153", "RHS (EN 10210-2):RHS100x50x5:441164" (+57 more) | descriptions: "FRQ{82A7443E-D5D7-4411-892A-A1E0254F1BBE}" | material: "Soletta metallica" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          1 x IFCMEMBER | type IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | object type "RHS160x80x5" | names: "RHS (EN 10210-2):RHS160x80x5:494863" | descriptions: "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          24 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS160x80x5" | object type "RHS160x80x5" | names: "RHS (EN 10210-2):RHS160x80x5:494888", "RHS (EN 10210-2):RHS160x80x5:494849", "RHS (EN 10210-2):RHS160x80x5:494862" (+21 more) | descriptions: "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" | material: "Soletta metallica" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          10 x IFCMEMBER | type IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | object type "RHS160x80x5" | names: "RHS (EN 10210-2):RHS160x80x5:494876", "RHS (EN 10210-2):RHS160x80x5:494874", "RHS (EN 10210-2):RHS160x80x5:494873" (+7 more) | descriptions: "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          2 x IFCMEMBER | type IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | object type "RHS160x80x5" | names: "RHS (EN 10210-2):RHS160x80x5:494875", "RHS (EN 10210-2):RHS160x80x5:494865" | descriptions: "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" | material: "Soletta metallica" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          2 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | object type "RHS180x100x5" | names: "RHS (EN 10210-2):RHS180x100x5:515463", "RHS (EN 10210-2):RHS180x100x5:515004" | descriptions: "FRQ{6673AEE9-34EB-43D3-AC48-8FBE5596D264}" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          12 x IFCBEAM | type IFCBEAMTYPE "RHS (EN 10210-2):RHS120x80x5" | object type "RHS120x80x5" | names: "RHS (EN 10210-2):RHS120x80x5:395457", "RHS (EN 10210-2):RHS120x80x5:395459", "RHS (EN 10210-2):RHS120x80x5:395461" (+9 more) | descriptions: "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
          13 x IFCMEMBER | type IFCMEMBERTYPE "IPE:IPE200" | object type "IPE200" | names: "IPE:IPE200:393952", "IPE:IPE200:429232", "IPE:IPE200:429242" (+10 more) | descriptions: "BP{D2F57514-A25F-4017-BC87-827E3E728933}" | material: "Acciaio strutturale - S235" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          1 x IFCMEMBER | type IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | object type "RHS160x80x5" | names: "RHS (EN 10210-2):RHS160x80x5:523816" | descriptions: "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" | material: "Acciaio strutturale - S235" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          1 x IFCMEMBER | type IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | object type "RHS160x80x5" | names: "RHS (EN 10210-2):RHS160x80x5:524004" | descriptions: "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" | material: "Acciaio strutturale - S235" | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities, ProfileProperties
          72 x IFCFASTENER | object type "Weld"
      IFCBUILDINGSTOREY "Livello" | long name "Livello" | object type "Livello:Estremità 8 mm" | elevation 0.
      IFCBUILDINGSTOREY "Livelloa" | long name "Livelloa" | object type "Livello:Estremità 8 mm" | elevation 300.

Types
  IFCFOOTINGTYPE "Muro di base:Generico - 400 mm" | FOOTING_BEAM | 6 occurrences
  IFCFOOTINGTYPE "Muro di base:Generico - 350 mm" | FOOTING_BEAM | 1 occurrence
  IFCRAMPTYPE "Pavimento:Rampa strutturale_CLS_2" | STRAIGHT_RUN_RAMP | 1 occurrence | material: "Calcestruzzo, gettato in opera" | property sets: Pset_RampCommon
  IFCWALLTYPE "Mura:Mura" | SOLIDWALL | 1 occurrence | material: "Muro di default"
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 4 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCRAMPTYPE "Pavimento:Rampa strutturale_CLS_1" | STRAIGHT_RUN_RAMP | 1 occurrence | material: "Calcestruzzo, gettato in opera" | property sets: Pset_RampCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 5 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro SHS (EN 10210-2):SHS120x5" | COLUMN | 13 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 11 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS120x80x5" | BEAM | 64 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "Barre circolari:RB 12" | MEMBER | 4 occurrences | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Barre circolari:RB 12" | MEMBER | 4 occurrences | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 2 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Pilastro RHS (EN 10210-2):RHS120x80x5" | COLUMN | 4 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_ColumnCommon
  IFCMEMBERTYPE "Barre circolari:RB 12" | MEMBER | 2 occurrences | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Barre circolari:RB 12" | MEMBER | 2 occurrences | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "RHS (EN 10210-2):RHS60x40x4" | MEMBER | 11 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | JOIST | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | JOIST | 5 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | JOIST | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | JOIST | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | JOIST | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | JOIST | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS100x50x5" | BEAM | 60 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | MEMBER | 1 occurrence | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS160x80x5" | BEAM | 24 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | MEMBER | 10 occurrences | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | MEMBER | 2 occurrences | material: "Soletta metallica" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "RHS (EN 10210-2):RHS180x100x5" | BEAM | 2 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "IPE:IPE200" | MEMBER | 13 occurrences | material: "Acciaio strutturale - S235" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | MEMBER | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "RHS (EN 10210-2):RHS160x80x5" | MEMBER | 1 occurrence | material: "Acciaio strutturale - S235" | property sets: Pset_MemberCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Informazioni sul progetto" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 94 objects (64 IFCBEAM, 30 IFCCOLUMN)
    Reference = "RHS120x80x5" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 60 objects (60 IFCBEAM)
    Reference = "RHS100x50x5" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 39 objects (24 IFCBEAM, 15 IFCMEMBER)
    Reference = "RHS160x80x5" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 13 objects (13 IFCCOLUMN)
    Reference = "SHS120x5" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 13 objects (13 IFCMEMBER)
    Reference = "IPE200" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 12 objects (12 IFCBEAM)
    Reference = "RHS180x100x5" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 12 objects (12 IFCMEMBER)
    Reference = "RB 12" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 11 objects (11 IFCMEMBER)
    Reference = "RHS60x40x4" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 6 more contents on 11 objects not shown
  Pset_FootingCommon | properties | on 6 objects (6 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generico - 400 mm" (IFCIDENTIFIER)
  Pset_FootingCommon | properties | on 1 object (1 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generico - 350 mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 6 objects (6 IFCFOOTING)
    Reference = "Generico - 400 mm" (IFCLABEL)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 1 object (1 IFCFOOTING)
    Reference = "Generico - 350 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 6 objects (6 IFCFOOTING)
    Reference = "Generico - 400 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 1 object (1 IFCFOOTING)
    Reference = "Generico - 350 mm" (IFCLABEL)
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 1.089194447408687 [SQUARE_METRE]
    Length = 91.952966313687213 [CENTI METRE]
    NetVolume = 0.43346088948173711 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 35.624247562527479 [SQUARE_METRE]
    Length = 3598.4088446997439 [CENTI METRE]
    NetVolume = 12.468486646884596 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 0.4789588914825994 [SQUARE_METRE]
    Length = 65.326719694656347 [CENTI METRE]
    NetVolume = 0.18936666711130146 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 3.2452200000000047 [SQUARE_METRE]
    Length = 327.8000000000003 [CENTI METRE]
    NetVolume = 1.2980879999999961 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 2.4658500563005274 [SQUARE_METRE]
    Length = 249.07576326267957 [CENTI METRE]
    NetVolume = 0.98634002252021225 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 1.0751211836866021 [SQUARE_METRE]
    Length = 215.02423673732042 [CENTI METRE]
    NetVolume = 0.43004847347464137 [CUBIC_METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 1.317960000000002 [SQUARE_METRE]
    Length = 156.90000000000009 [CENTI METRE]
    NetVolume = 0.52718399999999843 [CUBIC_METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Area = 0.033974922983496365 [SQUARE_METRE]
    Depth = 163.98003738141495 [CENTI METRE]
  Pset_RampCommon | properties | on 1 object (1 IFCRAMP)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Rampa strutturale_CLS_1" (IFCIDENTIFIER)
  Pset_RampCommon | properties | on 1 object (1 IFCRAMP)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Rampa strutturale_CLS_2" (IFCIDENTIFIER)
  Pset_RampCommon | properties | on 1 type object
    ThermalTransmittance = 2.6150000000000002 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RampCommon | properties | on 1 type object
    ThermalTransmittance = 1.7433333333333334 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RampFlightCommon | properties | on 1 object (1 IFCRAMP)
    Reference = "Rampa strutturale_CLS_1" (IFCIDENTIFIER)
    Slope = 4.6399436838957042 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_RampFlightCommon | properties | on 1 object (1 IFCRAMP)
    Reference = "Rampa strutturale_CLS_2" (IFCIDENTIFIER)
    Slope = 4.7322937396961811 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Vuoto rampa_1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 44 objects (44 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS100x50x5" (IFCIDENTIFIER)
    Roll = -15.58 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 300.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 43 objects (43 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS120x80x5" (IFCIDENTIFIER)
    Roll = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 300.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS160x80x5" (IFCIDENTIFIER)
    Roll = -3.5699999999999998 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 300.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS160x80x5" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 300.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS100x50x5" (IFCIDENTIFIER)
    Roll = 3.5699999999999998 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 300.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS180x100x5" (IFCIDENTIFIER)
    Roll = -105.58 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 300.08999999999997 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS100x50x5" (IFCIDENTIFIER)
    Roll = -15.58 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 302.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS120x80x5" (IFCIDENTIFIER)
    Roll = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 302.11000000000001 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_BeamCommon: 22 more contents on 26 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 64 objects (64 IFCBEAM)
    Reference = "RHS120x80x5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 60 objects (60 IFCBEAM)
    Reference = "RHS100x50x5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 24 objects (24 IFCBEAM)
    Reference = "RHS160x80x5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 12 objects (12 IFCBEAM)
    Reference = "RHS180x100x5" (IFCLABEL)
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    NetSurfaceArea = 2.603932131806173 [SQUARE_METRE]
    NetVolume = 0.0065760458579419076 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 9 objects (9 IFCBEAM)
    NetSurfaceArea = 1.577813706927456 [SQUARE_METRE]
    NetVolume = 0.0040161054922618579 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 9 objects (9 IFCBEAM)
    NetSurfaceArea = 1.577813706927456 [SQUARE_METRE]
    NetVolume = 0.0040161054922618466 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 8 objects (8 IFCBEAM)
    NetSurfaceArea = 1.577813706927456 [SQUARE_METRE]
    NetVolume = 0.0040161054922618709 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    NetSurfaceArea = 1.577813706927456 [SQUARE_METRE]
    NetVolume = 0.0040161054922617954 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    NetSurfaceArea = 2.6783312285991037 [SQUARE_METRE]
    NetVolume = 0.00676426411541289 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    NetSurfaceArea = 1.6121186932282989 [SQUARE_METRE]
    NetVolume = 0.0041035763165710769 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    NetSurfaceArea = 2.1127944546213029 [SQUARE_METRE]
    NetVolume = 0.0053492040321219238 [CUBIC_METRE]
  Qto_BeamBaseQuantities: 51 more contents on 96 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Mura" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Mura" (IFCIDENTIFIER)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    NetVolume = 218.15234382018579 [CUBIC_METRE]
  Pset_ColumnCommon | properties | on 30 objects (30 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS120x80x5" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 13 objects (13 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "SHS120x5" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 10 type objects
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfColumn | properties | on 30 objects (30 IFCCOLUMN)
    Reference = "RHS120x80x5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 13 objects (13 IFCCOLUMN)
    Reference = "SHS120x5" (IFCLABEL)
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    NetSurfaceArea = 5.180135282689367 [SQUARE_METRE]
    NetVolume = 0.013093095977833829 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    NetSurfaceArea = 5.180135282689367 [SQUARE_METRE]
    NetVolume = 0.013093095977833419 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    NetSurfaceArea = 5.180135282689367 [SQUARE_METRE]
    NetVolume = 0.0130930959778334 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    NetSurfaceArea = 4.2577352781564377 [SQUARE_METRE]
    NetVolume = 0.01078909597783421 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 2 objects (2 IFCCOLUMN)
    NetSurfaceArea = 1.6950021154575201 [SQUARE_METRE]
    NetVolume = 0.0042894148939654729 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 2 objects (2 IFCCOLUMN)
    NetSurfaceArea = 1.6950021154575201 [SQUARE_METRE]
    NetVolume = 0.004289414893965446 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 2 objects (2 IFCCOLUMN)
    NetSurfaceArea = 4.2577352781564377 [SQUARE_METRE]
    NetVolume = 0.010789095977834185 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 2 objects (2 IFCCOLUMN)
    NetSurfaceArea = 4.2577352781564377 [SQUARE_METRE]
    NetVolume = 0.010789095977834871 [CUBIC_METRE]
  Qto_ColumnBaseQuantities: 22 more contents on 23 objects not shown
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "IPE200" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 15.581815494575228 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 595.65000000000009 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS60x40x4" (IFCIDENTIFIER)
    Roll = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 15.581928542143627 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 533.50999999999999 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 10 objects (10 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS160x80x5" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 3.5652861146045787 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 192.97 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RB 12" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 34.075039800732171 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 362.31999999999999 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RB 12" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 34.075039800732164 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 362.31999999999999 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 3 objects (3 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RHS160x80x5" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 3.5652861146045742 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 192.97 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RB 12" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 28.507777626925229 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 341.51999999999998 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "RB 12" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 28.507777626925208 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 341.51999999999998 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon: 4 more contents on 3 objects not shown
  Qto_MemberBaseQuantities | quantities | on 4 objects (4 IFCMEMBER)
    NetSurfaceArea = 0.13009206490517777 [SQUARE_METRE]
    NetVolume = 0.00038957920977875945 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 4 objects (4 IFCMEMBER)
    NetSurfaceArea = 0.13009206490517777 [SQUARE_METRE]
    NetVolume = 0.00038957920977875955 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 3 objects (3 IFCMEMBER)
    NetSurfaceArea = 1.7708958680775972 [SQUARE_METRE]
    NetVolume = 0.0044685923977814132 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 3 objects (3 IFCMEMBER)
    NetSurfaceArea = 4.4823721677310679 [SQUARE_METRE]
    NetVolume = 0.01659921775294616 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 3 objects (3 IFCMEMBER)
    NetSurfaceArea = 1.8279033477605671 [SQUARE_METRE]
    NetVolume = 0.0037422891397033446 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 3 objects (3 IFCMEMBER)
    NetSurfaceArea = 4.4823721677310679 [SQUARE_METRE]
    NetVolume = 0.016599217752946999 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 3 objects (3 IFCMEMBER)
    NetSurfaceArea = 4.4823721677310679 [SQUARE_METRE]
    NetVolume = 0.016599217752947298 [CUBIC_METRE]
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetSurfaceArea = 0.12225064964181762 [SQUARE_METRE]
    NetVolume = 0.0003660560805306225 [CUBIC_METRE]
  Qto_MemberBaseQuantities: 23 more contents on 26 objects not shown
  ProfileProperties | properties | on 98 objects (98 IFCBEAM)
    Section = "AGB AB{7DFC1D4B-95DB-48DB-80AD-D36074A02721}" (IFCIDENTIFIER)
    SectionFamily = "{7DFC1D4B-95DB-48DB-80AD-D36074A02721}AGB AB" (IFCIDENTIFIER)
  ProfileProperties | properties | on 94 objects (64 IFCBEAM, 30 IFCCOLUMN)
    Section = "FRQ{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}" (IFCIDENTIFIER)
    SectionFamily = "{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}FRQ" (IFCIDENTIFIER)
  ProfileProperties | properties | on 78 objects (78 IFCBEAM)
    Section = "AGB AB{1D08A026-D2C0-42D8-B82A-53E07B6829BA}" (IFCIDENTIFIER)
    SectionFamily = "{1D08A026-D2C0-42D8-B82A-53E07B6829BA}AGB AB" (IFCIDENTIFIER)
  ProfileProperties | properties | on 60 objects (60 IFCBEAM)
    Section = "FRQ{82A7443E-D5D7-4411-892A-A1E0254F1BBE}" (IFCIDENTIFIER)
    SectionFamily = "{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}FRQ" (IFCIDENTIFIER)
  ProfileProperties | properties | on 39 objects (24 IFCBEAM, 15 IFCMEMBER)
    Section = "FRQ{FBBB44DB-2F88-44D3-BE58-6EF235688184}" (IFCIDENTIFIER)
    SectionFamily = "{ED1B2BEA-1066-44BD-B898-52A0D999EBC6}FRQ" (IFCIDENTIFIER)
  ProfileProperties | properties | on 24 objects (24 IFCBEAM)
    Section = "AGB AB{F3B0E60E-398C-4151-853C-68F2BDB22AF9}" (IFCIDENTIFIER)
    SectionFamily = "{1D08A026-D2C0-42D8-B82A-53E07B6829BA}AGB AB" (IFCIDENTIFIER)
  ProfileProperties | properties | on 13 objects (13 IFCCOLUMN)
    Section = "FRQ{C67B81B0-1E59-4DC6-8B30-115CE3698D26}" (IFCIDENTIFIER)
    SectionFamily = "{C67B81B0-1E59-4DC6-8B30-115CE3698D26}FRQ" (IFCIDENTIFIER)
  ProfileProperties | properties | on 13 objects (13 IFCMEMBER)
    Section = "BP{D2F57514-A25F-4017-BC87-827E3E728933}" (IFCIDENTIFIER)
    SectionFamily = "{D2F57514-A25F-4017-BC87-827E3E728933}BP" (IFCIDENTIFIER)
  ProfileProperties: 4 more contents on 31 objects not shown
  Pset_PlateCommon | properties | on 66 objects (66 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Non definito" (IFCIDENTIFIER)
    ThermalTransmittance (no value)
  Pset_BuildingStoreyCommon | properties | on 11 objects (11 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Estremità 8 mm" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Informazioni sul progetto" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 9 (IFCINTEGER)
    Reference = "Informazioni sul progetto" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Informazioni sul progetto" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Informazioni sul progetto" (IFCIDENTIFIER)